

TFSeries Tray Former

* Work Process: Film infeed → Thermal softening → Molding & Cooling → Die-cutting → Collection (stand alone mode) or to Tray Inserter (inline mode)
* Compact and small foot-print.
* Servo driven film movement for fast and precise film positioning.
* PLC controlled operation.
* User friendly touch control panel HMI.
* Safety enclosure.
* Multiple trays per mold possible.
* Seamless connection to Colamark’s tray insertion machine.

|  |  |
| --- | --- |
| **Model：** | **TF** |
| Name： | Series Tray Former |
| Capacity： | 20-40ppm |
| Weight： | 520kg |
| Electricity: | 380V 50Hz 2.5kW |
| Dimension(for reference)： | L)2,200×(W)1,738×(H)1,867 mm |
|  | |